Current configuration : 2762 bytes

!

version 12.1

no service timestamps log datetime msec

no service timestamps debug datetime msec

no service password-encryption

!

hostname Switch

!

!

!

!

username admin privilege 15 password 0 cisco

!

!

spanning-tree mode pvst

spanning-tree extend system-id

!

interface FastEthernet0/1

switchport access vlan 10

!

interface FastEthernet0/2

switchport access vlan 10

!

interface FastEthernet0/3

switchport access vlan 20

!

interface FastEthernet0/4

switchport access vlan 20

!

interface FastEthernet0/5

switchport access vlan 30

!

interface FastEthernet0/6

switchport access vlan 30

!

interface FastEthernet0/7

switchport access vlan 40

!

interface FastEthernet0/8

switchport access vlan 40

!

interface FastEthernet0/9

switchport access vlan 50

!

interface FastEthernet0/10

switchport access vlan 50

!

interface FastEthernet0/11

switchport access vlan 60

!

interface FastEthernet0/12

switchport access vlan 60

!

interface FastEthernet0/13

switchport access vlan 70

!

interface FastEthernet0/14

switchport access vlan 70

!

interface FastEthernet0/15

switchport access vlan 80

!

interface FastEthernet0/16

switchport access vlan 80

!

interface FastEthernet0/17

!

interface FastEthernet0/18

!

interface FastEthernet0/19

!

interface FastEthernet0/20

!

interface FastEthernet0/21

switchport access vlan 100

!

interface FastEthernet0/22

switchport access vlan 100

!

interface FastEthernet0/23

switchport access vlan 99

!

interface FastEthernet0/24

switchport access vlan 99

!

interface GigabitEthernet0/1

switchport mode trunk

!

interface GigabitEthernet0/2

!

interface Vlan1

no ip address

shutdown

!

interface Vlan10

description Created for use by Vendor 1

mac-address 0001.4208.d801

no ip address

!

interface Vlan20

description Created for use by Vendor 2

mac-address 0001.4208.d802

no ip address

!

interface Vlan30

description Created for use by Vendor 3

mac-address 0001.4208.d803

no ip address

!

interface Vlan40

description Created for use by Vendor 4

mac-address 0001.4208.d804

no ip address

!

interface Vlan50

description Created for use by Vendor 5

mac-address 0001.4208.d805

no ip address

!

interface Vlan60

description Created for use by Vendor 6

mac-address 0001.4208.d806

no ip address

!

interface Vlan70

description Created for use by Vendor 7

mac-address 0001.4208.d807

no ip address

!

interface Vlan80

description Created for use by Vendor 8

mac-address 0001.4208.d808

no ip address

!

interface Vlan99

description Created for use by Management

mac-address 0001.4208.d80a

no ip address

!

interface Vlan100

description Created for use by DCR

mac-address 0001.4208.d809

no ip address

!

banner motd ^CCourtney Hagen w0263284^C

!

!

!

line con 0

!

line vty 0 4

login local

line vty 5 15

login

!

!

!

!

end